Thanks to this tool we can easily see that, in this communication, only 2 protocols are involved

(ARP and TCP), and 2 IPs as well (192.168.56.1 and 192.168.56.102).

In order to have a better overview of the communication, we can go to “analyze / follow / TCP

stream ”, and this screen will show all of the messages.